  UWID: 300/J-19-6610-13730/0 [NT]        STATUS: Susp GAS
      LAHEE: DEV
  NAME: NORTHERN CROSS (YUKON) LIMITED CHANCE YT J-19
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Nrthrn Cross (Yukon) Lmtd [N043]   YT WID#: Y27
   ORIG OPER: Canoe River Expl Ltd [)233]            DA#: 0277

  GOVT KB: 518.6m     GL: 514.2m           MD:                   TVD: 1446.3m
  LOGS KB: 518.6m     GL: 514.2m                               FM@TD: Mhart_rv

                                           BH LAT:  66.14200 deg N
                                           BH LON: 137.54111 deg W

     SPUD: 1967/12/14  CMPL DRL:             DAYS:       RR: 1969/02/17
  DRL RIG: NABORS #1

     CASG: 0.35inch
           0.71inch
     LOGS: (SCH, Rm=0.710@135F) BHCS (246.3 ~ 1384.7m), IES (246.3 ~ 1385.0m),
           BHCS (1310.6 ~ 1442.3m), MCAL (1219.2 ~ 1444.4m), IES (1219.2 ~
           1444.4m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +518.6m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kprkin_ss     945.8  -427.2
  Kbrnhl_ck     432.5   +86.1          Kwhstn_rv     996.4  -477.8
  Kfish_brh     677.3  -158.7          Mhart_rv     1237.5  -718.9
  Kparkin       800.4  -281.8          T.D.         1446.3  -927.7
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.  1243.3 ~ 1260.3m Mhart_rv
  #02.  1260.7 ~ 1278.9m "  "
  #03.  1279.2 ~ 1293.9m "  "
  #04.  1337.5 ~ 1355.8m "  "
  #05.  1356.1 ~ 1372.5m "  "
  #06.  1389.9 ~ 1392.0m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1.  726.6 ~ 744.0m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     P Un: psi
     RMK: Rec. 535' wc mud. WAB / WAB rmn stdy TOT
  DST # 2. 1239.3 ~ 1260.7m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 140' condensate. GTS in 4mn mixed w/ mud. Skid tool 20' to btm.
          Lost apprx. 5bbls during skid.
  DST # 3. 1264.9 ~ 1279.2m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 50' mc condensate. SIAB. GTS in 1mn rmn stdy for 60mn., followed
          by mud & cond spr for last 90m
  DST # 4. 1278.9 ~ 1329.8m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final    2705  Mcf/d
     RMK: Rec. 140' sl $ gc mud. GTS in 4mn rmn stdy aft 2hr. TEOT
  DST # 5. 1330.1 ~ 1356.1m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final  178888  Mcf/d
     RMK: Rec. 175' oil. GIP. GTS in 3mn. MTS in 10mn.
  DST # 6. 1356.1 ~ 1372.8m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 1640' gy oil,360' swtr - salinity 1925ppm. GIB. GTS in 25mn TSTM.
  DST # 7. 1409.7 ~ 1446.3m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 380' mud. Misrun - Seat Failure.
  DST # 8. 1377.7 ~ 1392.9m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final   78583  Mcf/d
     RMK: Rec. 300' gy oc mud. GIP. GTS in 2mn.
  DST # 9. 1396.0 ~ 1446.3m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final     713  Mcf/d
     RMK: Rec. 465 gy mud,180' gy mc wtr,525' swtr. GIB G TS in 5mn.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
