  UWID: 300/C-24-6640-13745/0 [NT]        STATUS: Drld & ABD
      LAHEE: EXP
  NAME: EXXONMOBIL CANADA LTD. ELLEN YT C-24
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Exxonmobil Cda Ltd [E041]          YT WID#: Y13
   ORIG OPER: Socony Mobil Oil of Cda [&284]         DA#: 0144

  GOVT KB: 414.5m     GL: 410.0m           MD:                   TVD: 2174.4m
  LOGS KB: 414.5m     GL: 410.0m                               FM@TD: Mtuttle

                                           BH LAT:  66.55247 deg N
                                           BH LON: 137.83561 deg W

     SPUD: 1964/12/25  CMPL DRL:             DAYS:  100  RR: 1965/04/03
  DRL RIG: SOCONY MOBIL #4

     CASG: 0.28inch
           0.35inch
           0.51inch
           0.75inch
     LOGS: (SCH, Rm=1.140@122F) SRS (152.4 ~ 2170.2m), BHCS (237.1 ~ 2173.5m),
           MCAL (237.1 ~ 2173.8m), IES (237.1 ~ 2173.8m), CONTDIP (1219.2 ~
           2173.8m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +414.5m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kprkin_ss     998.2  -583.7
  Kbrnhl_ck     580.0  -165.5          Kwhstn_rv    1025.7  -611.2
  Kfish_brh     722.7  -308.2          Mtuttle      1471.6 -1057.1
  Kparkin       817.8  -403.3          T.D.         2174.4 -1759.9
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.  1597.2 ~ 1603.6m Mtuttle
  #02.  1603.6 ~ 1613.9m "  "
  #03.  1613.9 ~ 1623.4m "  "
  #04.  1623.4 ~ 1634.3m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1.  460.6 ~ 482.8m   Fm: Kcody_ck
     Source:  Government
                               Drill stem test MISRUN
     P Un: psi
     RMK: Misrun - seat failure.
  DST # 2.  722.1 ~ 746.5m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 1770' fld. Misrun Seat failure.
  DST # 3.  723.6 ~ 732.7m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 910' fld. WAB Misrun - seat failure.
  DST # 4. 1377.4 ~ 1423.7m  Fm: Kwhstn_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 405' oc fld. WAB dd in 20mn. Pkrs settled 10' TOT.
  DST # 5. 1508.2 ~ 1530.4m  Fm: Mtuttle
     Source:  Government
                               Drill stem test
     RMK: Rec. 530' sl gy fld. VWAB dd in 10mn.
  DST # 6. 1649.0 ~ 1667.0m  Fm: Mtuttle
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 210' fld. VWAB dd in 35mn. Misrun - tool plugged.
  DST # 7. 1649.0 ~ 1676.7m  Fm: Mtuttle
     Source:  Government
                               Drill stem test MISRUN
     RMK: No rec. Misrun - unable to reach btm. Bridge @ 3150'.
  DST # 8. 1649.0 ~ 1676.7m  Fm: Mtuttle
     Source:  Government
                               Drill stem test
     RMK: Rec. 230' fld. WAB dd in 10mn.
  DST # 9. 1886.7 ~ 1912.9m  Fm: Mtuttle
     Source:  Government
                               Drill stem test
     RMK: Rec. 15' sl gc mud. VWAB dd in 50mn.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
