  UWID: 300/D-77-6550-13700/0 [NT]        STATUS: Drld & ABD
      LAHEE: EXP
  NAME: CHEVRONTEXACO BLACKSTONE YT D-77
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Chevrontexaco [C150]               YT WID#: Y4
   ORIG OPER: California Standard Comp [!813]        DA#: 0109

  GOVT KB: 645.0m     GL: 640.1m           MD:                   TVD: 4028.5m
  LOGS KB: 518.2m     GL: 513.3m                               FM@TD: Ofrnk_mtn

                                           BH LAT:  65.76967 deg N
                                           BH LON: 137.24856 deg W

     SPUD: 1962/03/10  CMPL DRL:             DAYS:  305  RR: 1963/01/08
  DRL RIG: TRINITY CAN. #5

     CASG: 0.28inch
           0.35inch
           0.51inch
     LOGS: (SCH, Rm=0.470@219F) S (60.7 ~ 599.8m), MCAL (60.7 ~ 599.8m), IES
           (60.7 ~ 599.8m), LL (601.1 ~ 1847.1m), S (601.1 ~ 1847.1m), LL
           (1616.4 ~ 4023.4m), S (1616.4 ~ 4023.4m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +645.0m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Mhart_rv      287.7  +357.3          Dgossage     1262.5  -617.5
  Dimperial     819.3  -174.3          Droad_rv     2209.2 -1564.2
  Dcanol       1083.9  -438.9          Ofrnk_mtn    2827.3 -2182.3
  Dhume        1101.5  -456.5          T.D.         4028.5 -3383.5
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.  1117.1 ~ 1130.2m Dhume
  #02.  1595.0 ~ 1605.1m Dgossage
  #03.  1766.0 ~ 1774.5m "  "
  #04.  2475.3 ~ 2493.3m Droad_rv
  #05.  2834.6 ~ 2846.2m Ofrnk_mtn
  #06.  3304.0 ~ 3322.3m "  "
  #07.  3900.8 ~ 3905.1m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1. 1494.7 ~ 1616.4m  Fm: Dgossage
     Source:  Government
                               Drill stem test
     P Un: psi
     RMK: Rec 190' mud. TAB < WAB > TO
  DST # 2. 1737.7 ~ 1774.5m  Fm: Dgossage
     Source:  Government
                               Drill stem test
     RMK: Rec 400' mc s wtr, 2600 sy $ wtr. GAB
  DST # 3. 2011.7 ~ 2061.7m  Fm: Dgossage
     Source:  Government
                               Drill stem test
     RMK: Rec 540' wc mud, 3890 wtr
  DST # 4. 2499.4 ~ 2514.9m  Fm: Droad_rv
     Source:  Government
                               Drill stem test
     RMK: Rec 40' mud
  DST # 5. 2650.8 ~ 2660.0m  Fm: Droad_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 570' wtr CSH
  DST # 6. 2889.5 ~ 3021.5m  Fm: Ofrnk_mtn
     Source:  Government
                               Drill stem test
     RMK: Rec. 2500' wtr CSH, 5540 mc sl gc s wtr
  DST # 7. 2807.2 ~ 2852.9m  Fm: Ofrnk_mtn
     Source:  Government
                               Drill stem test
     RMK: Rec. 2245' wtr CSH, 30' mud
  DST # 8. 3811.2 ~ 3859.4m  Fm: Ofrnk_mtn
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun- mud dropped. Pkr seat failed. Rec 5510' wtr CSH
  DST # 9. 3974.0 ~ 4028.5m  Fm: Ofrnk_mtn
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - rig broke down.
  DST #10. 3974.0 ~ 4028.5m  Fm: Ofrnk_mtn
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - pkr seat failed. WIP dd in 1mn
  DST #11. 3974.6 ~ 4028.5m  Fm: Ofrnk_mtn
     Source:  Government
                               Drill stem test MISRUN
     RMK: WAB dd in 30mn. No rec. Pkr stuck when pulling loose. Misrun
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
