  UWID: 300/B-34-6610-13645/0 [NT]        STATUS: Drld & ABD
      LAHEE: EXP
  NAME: EXXONMOBIL CANADA LTD. BIRCH YT B-34
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Exxonmobil Cda Ltd [E041]          YT WID#: Y17
   ORIG OPER: Socony Mobil Oil of Cda [&284]         DA#: 0156

  GOVT KB: 667.5m     GL: 663.5m           MD:                   TVD: 1649.9m
  LOGS KB: 667.5m     GL: 663.5m                               FM@TD: Mhart_rv

                                           BH LAT:  66.05086 deg N
                                           BH LON: 136.85486 deg W

     SPUD: 1965/04/08  CMPL DRL:             DAYS:   62  RR: 1965/06/08
  DRL RIG: PARKER #10

     CASG: 0.35inch
           0.51inch
     LOGS: (SCH, Rm=0.770@97F) CONTDIP (1082.0 ~ 1504.8m), BHCS (182.9 ~
           1534.1m), MCAL (182.9 ~ 1535.6m), IES (182.9 ~ 1535.9m), SRS (182.9 ~
           1646.8m), BHCS (1463.0 ~ 1646.8m), IES (1463.0 ~ 1647.1m), MCAL
           (1463.0 ~ 1647.1m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +667.5m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kparkin       Cased                  PNettrain     522.4  +145.1
  Kprkin_ss      80.5  +587.0          PNblackie     815.6  -148.1
  Kwhstn_rv     118.9  +548.6          Mhart_rv     1160.4  -492.9
  PRjung_ck     290.5  +377.0          T.D.         1649.9  -982.4
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.   287.7 ~ 293.8m  PRjung_ck
  #02.   392.9 ~ 399.0m  "  "
  #03.   658.7 ~ 661.7m  PNettrain
  #04.   707.1 ~ 710.2m  "  "
  #05.  1095.5 ~ 1098.5m PNblackie
  #06.  1408.8 ~ 1411.5m Mhart_rv
  #07.  1491.4 ~ 1492.6m "  "
  #08.  1538.3 ~ 1539.8m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1.  289.6 ~ 293.8m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     P Un: psi
     RMK: Rec. 20' wc mud. FAB > WAB
  DST # 2.  293.8 ~ 354.5m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 120' sly wc mud. 7' flare. SAB GTS in 5mn
  DST # 3.  354.5 ~ 405.1m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 220' mud. WAB dd in 20mn
  DST # 4.  487.7 ~ 509.9m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 15' mud. WAB TOT Faint trace of oil
  DST # 5.  701.0 ~ 707.1m   Fm: PNettrain
     Source:  Government
                               Drill stem test
     RMK: Rec. 180' sly wc mud,700' sly mc swtr,650' cln sy wtr. SAB > FAB TOT
  DST # 6. 1350.3 ~ 1371.9m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 300' gc $ wtr. GAB GTS in 4mn, MTS in 35mn. Mud dropped 4'. Tool
          waschased 12' during test.
  DST # 7.  453.5 ~ 464.8m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec 700' mud. FAB > WAB. Mud dropped 35' Pkr settled 3' & tool chased
          8'.
  DST # 8.  458.7 ~ 463.3m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 270' mud, 420' fr wtr. FAB > WAB. Mud dropped 20', tool was
          chased 12'.
  DST # 9. 1583.4 ~ 1649.9m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final  260524  Mcf/d
     RMK: Rec. 330' gc mud. GAB GTS in 1mn. Mud dropped 2' and tool was chased
          2'.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
