  UWID: 300/G-08-6610-13730/0 [NT]        STATUS: Susp OIL
      LAHEE: EXP
  NAME: NORTHERN CROSS (YUKON) LIMITED CHANCE YT G-08
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Nrthrn Cross (Yukon) Lmtd [N043]   YT WID#: Y12
   ORIG OPER: Socony Mobil Oil of Cda [&284]         DA#: 0143

  GOVT KB: 524.2m     GL: 518.8m           MD:                   TVD: 1579.8m
  LOGS KB: 524.2m     GL: 518.8m                               FM@TD: Mhart_rv

                                           BH LAT:  66.12169 deg N
                                           BH LON: 137.51411 deg W

     SPUD: 1964/12/04  CMPL DRL:             DAYS:   77  RR: 1965/02/18
  DRL RIG: PARKER #10

     CASG: 0.35inch
           0.51inch
     LOGS: (SCH, Rm=0.780@100F) SRS (246.9 ~ 1502.7m), CONTDIP (1082.0 ~
           1504.8m), ML (246.9 ~ 1505.4m), IES (246.9 ~ 1505.4m), BHCS (246.9 ~
           1505.7m), BHCS (1498.1 ~ 1577.9m), IES (1498.1 ~ 1579.5m), ML (1498.1
           ~ 1579.5m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +524.2m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kprkin_ss     913.2  -389.0
  Kbrnhl_ck     458.7   +65.5          Kwhstn_rv     970.8  -446.6
  Kfish_brh     676.4  -152.2          Mhart_rv     1194.5  -670.3
  Kparkin       768.1  -243.9          T.D.         1579.8 -1055.6
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  PERFS/TREATMENTS
  #01.  Bul    1339.0 ~ 1342.0m                                     Mhart_rv
  #02.  Bul    1348.0 ~ 1359.0m                                     "  "
  #03.  Trtmnt 1339.0 ~ 1359.0m                                     "  "
  #04.  Trtmnt 1339.0 ~ 1359.0m                                     "  "
  #05.  Bul    1364.0 ~ 1365.0m                                     "  "
  #06.  Bul    1366.0 ~ 1367.0m                                     "  "
  #07.  Bul    1368.0 ~ 1369.0m                                     "  "
  #08.  Bul    1383.0 ~ 1384.0m                                     "  "
  #09.  Trtmnt 1364.0 ~ 1388.0m                                     "  "
  #10.  Trtmnt 1364.0 ~ 1388.0m                                     "  "
  #11.  Bul    1388.0 ~ 1389.0m                                     "  "
  #12.  Bul    1395.0 ~ 1395.0m                                     "  "
  #13.  Bul    1420.0 ~ 1420.0m                                     "  "
  #14.  Bul    1423.0 ~ 1424.0m                                     "  "
  #15.  Trtmnt 1418.0 ~ 1427.0m                                     "  "
  #16.  Trtmnt 1418.0 ~ 1427.0m                                     "  "
  #17.  BrPlug 1427.0 ~ 1428.0m                                     "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.   695.9 ~ 708.4m  Kfish_brh
  #02.  1101.2 ~ 1104.3m Kwhstn_rv
  #03.  1197.9 ~ 1207.0m Mhart_rv
  #04.  1299.4 ~ 1302.4m "  "
  #05.  1340.2 ~ 1343.3m "  "
  #06.  1384.4 ~ 1390.5m "  "
  #07.  1530.1 ~ 1530.7m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1.  673.6 ~ 688.8m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final  118762  Mcf/d
     P Un: psi
     RMK: Rec.2' mud. GAB GTS in 2mn. MTS in 25mn. Blew gas aft 155 mn.
  DST # 2.  691.9 ~ 710.2m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: 180' mud. FAB GTS in 12mn 10' flr. TSTM
  DST # 3. 1194.8 ~ 1207.0m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 170' gc mud. WAB TOT. Tool was chased 6' during the test period.
  DST # 4. 1295.4 ~ 1299.1m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 75' $ gc fld. WAB < FAB GTS in 54mn 2' flr. TSTM. Misrun, tool
          plgd. 14' of fill on btm.
  DST # 5. 1289.3 ~ 1302.4m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 160' blk $ gc fld. GAB > sl TOT GTS in 7mn TSTM
  DST # 6. 1333.5 ~ 1340.2m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 1180' oil. GAB > sl TOT. GTS in 3mn. TSTM. Tool was chased 9'
          during the test period.
  DST # 7. 1302.4 ~ 1333.5m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 40' gy oc fld. GSAB > dd in 60mn. Mud drop0ped 1.5' during test
          period. Tool chased 10' d test.
  DST # 8. 1340.2 ~ 1343.3m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun Unable to reach btm. Btm, 30' fill on btm.
  DST # 9. 1340.2 ~ 1346.3m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 140' oil. VWAB GTS in 32mn. Flr on 2" riser 6' - 8'.
  DST #10. 1345.1 ~ 1379.2m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 410' oil,100' mc oil. OTS in SAB dd in 40mn / SAB TOT. Mud
          dropped 6' during the test period.
  DST #11. 1379.2 ~ 1384.4m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final    5856  Mcf/d
     RMK: No Rec. SAB GTS in 5mn > aft 10mn, stdy TOT TSTM.
  DST #12. 1385.9 ~ 1392.9m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final    5324  Mcf/d
     RMK: Rec. 270' gc mud,90' mc oil. GAB stdy TOT.
  DST #13. 1417.3 ~ 1434.4m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test MISRUN
     GTS:         Flo:Max           Final   30418  Mcf/d
     RMK: Rec. 450' gy mud. SAB GTS in 8mn. Misrun, did not obtain SI pressures.
  DST #14. 1435.0 ~ 1462.1m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 4670' blk $ oflk swtr. GAB GTS in 8mn. Blk $ WTS in 55mn. TSTM
  DST #15. 1462.1 ~ 1506.9m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 740' gc $ fld. SAB > GTS in 5mn. TSTM. Good test.
  DST #16. 1495.3 ~ 1530.7m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 630' filt wc gc fld. GAB > WAB GTS in 4mn TSTM
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
