  UWID: 300/I-13-6610-13745/0 [NT]        STATUS: Drld & ABD
      LAHEE: EXP
  NAME: CHEVRONTEXACO E PORCUPINE YT I-13
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Chevrontexaco [C150]               YT WID#: Y38
   ORIG OPER: Chevron Cda Rsrcs Lmtd [#137]          DA#: 0498

  GOVT KB: 507.5m     GL: 501.4m           MD:                   TVD: 2439.6m
  LOGS KB: 507.5m     GL: 501.4m                               FM@TD: Mhart_rv

                                           BH LAT:  66.04306 deg N
                                           BH LON: 137.78278 deg W

     SPUD: 1971/02/10  CMPL DRL:             DAYS:   82  RR: 1971/05/02
  DRL RIG: GENERAL PETROLEUM #14

     CASG: 0.63inch CND
           0.79inch CND
           0.35inch
     LOGS: (SCH, Rm=1.464@154F) BHCS (21.3 ~ 237.4m), MCAL (21.3 ~ 239.6m), IES
           (21.3 ~ 239.9m), VS (1097.3 ~ 1219.2m), SNP (1097.3 ~ 1219.2m), FDC
           (1767.8 ~ 2437.8m), DILL (242.9 ~ 2437.8m), SNP (1767.8 ~ 2437.8m),
           BHCS (242.9 ~ 2438.7m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +507.5m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kwhstn_rv    1356.7  -849.2
  Kbrnhl_ck     778.2  -270.7          PNettrain    1822.7 -1315.2
  Kfish_brh    1105.2  -597.7          Mhart_rv     2137.9 -1630.4
  Kparkin      1198.5  -691.0          T.D.         2439.6 -1932.1
  Kprkin_ss    1349.7  -842.2
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.  1115.0 ~ 1132.9m Kfish_brh
  #02.  1829.4 ~ 1834.9m PNettrain
  #03.  1834.9 ~ 1841.0m "  "
  #04.  1868.4 ~ 1875.4m "  "
  #05.  2303.7 ~ 2304.6m Mhart_rv
  #06.  2387.5 ~ 2388.4m "  "
  #07.   320.0 ~ 2390.2m Kprkin_ss
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1. 1103.4 ~ 1115.0m  Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     P Un: psi
     RMK: Rec. 465' sl wc mud. GAB dd in 10mn / WAB TO > dd in 10mn
  DST # 2. 1109.2 ~ 1162.2m  Fm: Kfish_brh
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 1085' mud. FAB TO / WAB < FAB dd. Tool plugged off on IF. Test
          considered misrun.
  DST # 3. 1106.1 ~ 1162.2m  Fm: Kfish_brh
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 585' mud. WAB dd in 5mn / VWAB dd in 5mn. Tool plugged - test
          considered misrun.
  DST # 4. 1821.8 ~ 1845.0m  Fm: PNettrain
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 1290' mud. SAB TOT. Misrun no pkr seat. Plug dropped slwly TOT
          150'.
  DST # 5. 2377.4 ~ 2439.6m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final    1810  Mcf/d
     RMK: Rec. 186' bl $ mud. GAB TOT / GTS in 5mn
  DST # 6.  758.0 ~ 781.8m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 558' gc mud. WAB TOT. Btm pkr did not hold - lost 10' through by-
          pass on PF. Mud was lost.
  DST # 7. 1823.3 ~ 1847.1m  Fm: PNettrain
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final     461  Mcf/d
     RMK: Rec. 190' gc mud,2320' swtr. Salinity for wtr 39300ppm. GTS in 10mn
          Average Perm indicated by SI pre
  DST # 8.  758.0 ~ 781.8m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 125' mud. GIP > WAB Tool plugged immediately. Misrun
  DST # 9.  757.7 ~ 776.6m   Fm: Kcody_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 30' filt wtr,120' mud. GIP SAB / SAB > sl TOT. Very Low
          Permibility indicated by SI pressures.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
