These files accompany the Dawson Land Use Planning Mineral Potential Assessment, Yukon Geological Survey Miscellaneous Report 8.

When referring to this document please use the following citation:
Kilby, W.E., 2013. Dawson Land Use Planning Mineral Potential Assessment. Yukon Geological Survey, Miscellaneous Report 8, 124 p., including appendices.

© Department of Energy, Mines and Resources, Government of Yukon

DIGITAL APPENDIX (Separate digital file)

The digital appendix is provided as a separate digital file associated with YGS Miscellaneous Report 8. The digital products are provided in a variety of formats. Some of the contents are historic information compiled from the previous mineral potential assessment processing used in this compilation while others are products generated during this compilation effort.

Shapefiles

	Deposits_by_Tract- A Shapefile containing the number of deposits of each type that were estimated by the expert estimators at the four estimation workshops. The deposit values are in estimated deposits per km2. The spatial information is provided in the Yukon Albers projection on the NAD 83 Datum.

	Commodity_by_Tract- A Shapefile containing the mass of each type of commodity that was estimated by the expert estimators. The mass values are in tonnes per km2. The spatial information is provided in the Yukon Albers projection on the NAD 83 Datum.  Those fields labeled with a “PLUS” contain the known commodity tonnages as well as the estimated values.

	Confidence_by_Tract- A Shapefile containing the confidence values for each tract calculated from the expert estimators individual evaluations made during the workshops.

	CUR_GIPV- A Shapefile containing the tabulated GIPV of all the commodities contained in the tracts of the Dawson Assessment Area. The ranking results are provided for all the calculation types. The GIPV units are dollars per km2. The commodity prices are from the Current Price List. The spatial information is provided in the Yukon Albers projection on the NAD 83 Datum.

	YT_GIPV- A Shapefile containing the tabulated GIPV of all the commodities contained in the tracts of the Dawson Assessment Area. The ranking results are provided for all the calculation types. The GIPV units are dollars per km2. The commodity prices are from the Yukon Price List. The spatial information is provided in the Yukon Albers projection on the NAD 83 Datum.

	BC_GIPV- A Shapefile containing the tabulated GIPV of all the commodities contained in the tracts of the Dawson Assessment Area. The ranking results are provided for all the calculation types. The GIPV units are dollars per km2. The commodity prices are from the BC Price List. The spatial information is provided in the Yukon Albers projection on the NAD 83 Datum.

Deposit Models
This appendix contains the digital deposit model files (*.DAT and *.DEF) for all the models used in the Dawson Assessment.
	
	*.DAT file- a tabular text file containing a list of all the known deposits that make up the digital model.
	*.DEF file- a text file that contains the model number, its name and a coded list of all the known deposits that make up the digital deposit model.

Estimation Files
This section of the digital appendix contains the scanned estimation coding sheets for the tracts involved in the Dawson Assessment. The coding sheets are in PDF format. They are provided in directories for each workshop (North, Peel, Selwyn, South and White Gold). In addition to the coding sheets the files containing the digitized data from the coding sheets are also included in the appropriate directories.

Keyhole Markup File
Keyhole markup file (KML) that can be viewed with the Google Earth™ viewer.

Software
Mark3B.BAS
Phase1.BAS
Raw2Mark.BAS
Sim-Valu.EXE
price lists
Depnum.BAS
ComSum.BAS



APPENDIX: Yukon Albers Projection
ESPG:3578  (European Petroleum Survey Group code)

Projection: ALBERS
Datum: NAD83
Zunits: NO
Units: METRES
Spheroid: GRS1980
Xshift: 0.0000000000
Yshift: 0.0000000000

Parameters
1st Standard Parallel: 61 40 0.00
2nd Standard Parallel:	68 0 0.00
Central Meridian: -132 30 0.00
Latitude of Proj. Origin: 50 0 0.00
False Easting: 500000.0 m
False Northing: 500000.0 m