  UWID: 300/D-22-6620-13730/0 [NT]        STATUS: Drld & ABD
      LAHEE: EXP
  NAME: EXCO ENERGY CHANCE YT D-22
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Exco Enrg Ltd [E009]               YT WID#: Y66
   ORIG OPER: Exco Enrg Ltd [)288]                   DA#: 1209

  GOVT KB: 535.4m     GL: 531.5m           MD:                   TVD: 1830.0m
  LOGS KB: 535.4m     GL: 531.5m                               FM@TD: Mford_lk

                                           BH LAT:  66.18503 deg N
                                           BH LON: 137.59247 deg W

     SPUD: 1985/03/01  CMPL DRL:             DAYS:   40  RR: 1985/04/09
  DRL RIG: CUSTOM #94

     CASG: 339.0mm CND
           20.0mm CND
           244.0mm SRF
           244.0mm SRF
           9.0mm
           140.0mm
     LOGS: (COM, Rm=3.170@38C) ML (459.5 ~ 1818.9m), CDCN (459.5 ~ 1821.8m),
           DILL (459.5 ~ 1829.2m), COMP (459.5 ~ 1829.2m), S (459.2 ~ 1829.6m),
           D (685.8 ~ 2114.7m), DILL (291.1 ~ 2118.4m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +535.4m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kwhstn_rv    1059.3  -523.9
  Kbrnhl_ck     540.0    -4.6          Mhart_rv     1318.8  -783.4
  Kfish_brh     785.7  -250.3          Mford_lk     1815.2 -1279.8
  Kparkin       878.8  -343.4          T.D.         1830.0 -1294.6
  Kprkin_ss    1020.5  -485.1
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1. 1807.5 ~ 1829.4m  Fm: Mford_lk
     Source:  Government
                               Drill stem test
     P Un: kPa
     RMK: Rec. 420' my sly gy wtr. FIB slwly > TOT
  DST # 1. 1433.0 ~ 1436.0m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 868m sour swtr,10 swtr. Guage 545 show stairstepping on PF & part
          of ISI.. 70 L Inhibiton & Wtr
  DST # 2. 1538.0 ~ 1554.0m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - No pkr seat.
  DST # 2.  719.3 ~ 749.8m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - seat failure. Tools were skidding slwly the first couple of
          tries, total 3'.Mud dropped slw
  DST # 3. 1538.0 ~ 1554.0m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 3m my INHIB - 140 L Inhib & wtr.
  DST # 3.  717.8 ~ 749.8m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - set pkr and mud dropped imm.
  DST # 4.  786.0 ~ 789.0m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: Rec. 21m mc wtr.
  DST # 4.  719.6 ~ 748.0m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - pkr did not hold. Opened tool and slid about 7'.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests, Cores or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
