  UWID: 300/M-59-6600-13700/0 [NT]        STATUS: Susp GAS
      LAHEE: EXP
  NAME: NORTHERN CROSS (YUKON) LIMITED BLACKIE #1 YT M-59
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Nrthrn Cross (Yukon) Lmtd [N043]   YT WID#: Y9
   ORIG OPER: Socony Mobil Oil of Cda [&284]         DA#: 0125

  GOVT KB: 562.1m     GL: 557.4m           MD:                   TVD: 1931.8m
  LOGS KB: 562.1m     GL: 557.5m                               FM@TD: Mhart_rv

                                           BH LAT:  65.98125 deg N
                                           BH LON: 137.18359 deg W

     SPUD: 1963/12/11  CMPL DRL:             DAYS:  108  RR: 1964/03/27
  DRL RIG: SOCONY MOBIL #4

     CASG: 0.51inch
           0.71inch
     LOGS: (SCH, Rm=0.865@153F) GR (18.3 ~ 336.2m), VS (265.8 ~ 1905.0m), SG
           (336.2 ~ 1905.0m), IES (336.2 ~ 1907.1m), MCAL (336.2 ~ 1907.4m), GR
           (1905.0 ~ 1931.2m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +562.1m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kwhstn_rv     428.5  +133.6
  Kbrnhl_ck     112.8  +449.3          PRjung_ck     576.1   -14.0
  Kfish_brh     265.2  +296.9          PNettrain     891.5  -329.4
  Kparkin       327.7  +234.4          Mhart_rv     1574.0 -1011.9
  Kprkin_ss     419.1  +143.0          T.D.         1931.8 -1369.7
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.   597.4 ~ 603.5m  PRjung_ck
  #02.   644.7 ~ 649.2m  "  "
  #03.   649.8 ~ 656.4m  "  "
  #04.   656.5 ~ 668.7m  "  "
  #05.   718.4 ~ 724.5m  "  "
  #06.   902.8 ~ 905.9m  PNettrain
  #07.  1188.7 ~ 1191.8m "  "
  #08.  1600.5 ~ 1603.1m Mhart_rv
  #09.  1902.0 ~ 1905.0m "  "
  #10.  1917.8 ~ 1927.1m "  "
  #11.  1927.1 ~ 1931.8m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1.  640.7 ~ 649.8m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final      99  Mcf/d
     P Un: psi
     RMK: Rec. 150' mud. Tight Hole.GTS imm < & stable. Choke @ tool 1/2"; 40 -
          45' flr.
  DST # 2.  649.8 ~ 656.5m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final      51  Mcf/d
     RMK: Rec. 120' mud. Tight Hole. GTS imm <. Choke at tool 1/2".
  DST # 3.  656.5 ~ 669.0m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final       3  Mcf/d
     RMK: Rec. 100' mud. GIP GTS 19mn. 5' fill on tbtm skidded through. ISI & IF
          not reliable.
  DST # 4.  655.3 ~ 724.8m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 90' mud,180' my wtr,1480' fr wtr. GIP GTS in 35mn TSTM. 8' fill
          on btm - skidded through.
  DST # 5.  749.8 ~ 759.0m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 10' mud. WIP. Misrun. Tool possibly plugged. Checked tool nothing
          wrong.
  DST # 6.  749.8 ~ 759.0m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Rec. 40' mud. WIP TAB dd aft 8mn. Misrun Pulled pkr loose aft 80mn
          flow & reset. Tool plugged.
  DST # 7.  749.2 ~ 759.0m   Fm: PRjung_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 140' wc mud, 885' my wtr. GIP FAB > TOF. Tight Hole.
  DST # 8. 1770.9 ~ 1783.1m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 40' mud. VWAB dd in 56mn. Rmn stdy for 34mn . Had to drop 3 bars
          before tool opened.
  DST # 9. 1895.2 ~ 1931.8m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 1850' gc mud. FAB < GAB dd aft 10mn < sl GTS in 42mn - gas not
          measured.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No Perfs/Treatments, IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
