  UWID: 300/M-08-6610-13730/0 [NT]        STATUS: Susp GAS
      LAHEE: OTH
  NAME: NORTHERN CROSS (YUKON) LIMITED CHANCE YT NO 1 M-08
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
   CURR OPER: Nrthrn Cross (Yukon) Lmtd [N043]   YT WID#: Y2
   ORIG OPER: Wstrn Mnrls Ltd [(096]                 DA#: 0058

  GOVT KB: 539.2m     GL: 534.0m           MD:                   TVD: 2635.9m
  LOGS KB: 539.2m     GL: 534.0m                               FM@TD: Mford_lk

                                           BH LAT:  66.12942 deg N
                                           BH LON: 137.52425 deg W

     SPUD: 1959/05/30  CMPL DRL:             DAYS:  362  RR: 1960/05/25
  DRL RIG: UNKNOWN

     CASG: 0.79inch CND
           0.35inch
     LOGS: (SCH, Rm=1.400@118F) TEMPL (45.7 ~ 611.1m), TEMPL (1385.9 ~ 1416.4m),
           S (609.6 ~ 2446.9m), GRN (88.4 ~ 2447.5m), ML (48.5 ~ 2474.4m), EL
           (48.2 ~ 2474.7m)
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  FORMATION TOPS
   geoSCOUT REF ELEV: +539.2m
  FORMATION       TVD    ELEV          FORMATION       TVD    ELEV
  Kcody_ck      Cased                  Kwhstn_rv     998.8  -459.6
  Kbrnhl_ck     459.3   +79.9          Mhart_rv     1230.2  -691.0
  Kfish_brh     702.3  -163.1          Mchance      1297.8  -758.6
  Kparkin       795.2  -256.0          Mford_lk     2040.9 -1501.7
  Kprkin_ss     942.4  -403.2          T.D.         2635.9 -2096.7
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  PERFS/TREATMENTS
  #01.  Jet 1320.0 ~ 1321.0m                                        Mchance
  #02.  Jet 1323.0 ~ 1323.0m                                        "  "
  #03.  Jet 1325.0 ~ 1325.0m                                        "  "
  #04.  Jet 1328.0 ~ 1329.0m                                        "  "
  #05.  Jet 1329.0 ~ 1330.0m                                        "  "
  #06.  Jet 1330.0 ~ 1331.0m                                        "  "
  #07.  Jet 1330.0 ~ 1331.0m                                        "  "
  #08.  Jet 1332.0 ~ 1332.0m                                        "  "
  #09.  Jet 1332.0 ~ 1333.0m                                        "  "
  #10.  Jet 1335.0 ~ 1335.0m                                        "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  CORES
  #01.   382.5 ~ 389.8m  Kcody_ck
  #02.   390.1 ~ 400.8m  "  "
  #03.   401.1 ~ 411.2m  "  "
  #04.   620.3 ~ 624.2m  Kbrnhl_ck
  #05.   709.0 ~ 713.8m  Kfish_brh
  #06.   735.8 ~ 740.7m  "  "
  #07.  1044.9 ~ 1054.0m Kwhstn_rv
  #08.  1234.4 ~ 1239.6m Mhart_rv
  #09.  1265.8 ~ 1267.4m "  "
  #10.  1296.9 ~ 1303.6m Mchance
  #11.  1303.9 ~ 1314.6m "  "
  #12.  1314.9 ~ 1326.8m "  "
  #13.  1327.1 ~ 1333.2m "  "
  #14.  1337.2 ~ 1338.7m "  "
  #15.  1339.3 ~ 1341.7m "  "
  #16.  1384.4 ~ 1386.2m "  "
  #17.  1392.3 ~ 1400.9m "  "
  #18.  1401.2 ~ 1403.3m "  "
  #19.  1445.7 ~ 1448.7m "  "
  #20.  1581.9 ~ 1585.0m "  "
  #21.  1587.4 ~ 1589.2m "  "
  #22.  1685.8 ~ 1687.4m "  "
  #23.  1838.9 ~ 1844.3m "  "
  #24.  1854.7 ~ 1860.2m "  "
  #25.  1946.1 ~ 1953.8m "  "
  #26.  2002.8 ~ 2011.7m "  "
  #27.  2136.6 ~ 2141.8m Mford_lk
  #28.  2378.4 ~ 2386.3m "  "
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  DSTS/FORMATION TESTS
  DST # 1.  413.6 ~ 423.7m   Fm: Kcody_ck
     Source:  Government
                               Drill stem test
     P Un: psi
     RMK: Rec. 10' mud. WIP, WAB
  DST # 2.  612.3 ~ 620.3m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - shoulder failed.
  DST # 3.  615.4 ~ 620.3m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - shoulder failed.
  DST # 4.  607.2 ~ 620.3m   Fm: Kbrnhl_ck
     Source:  Government
                               Drill stem test
     RMK: Rec. 10' mud. WIP dd in 20mn
  DST # 5.  697.7 ~ 709.0m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: Rec. 100' mud. GIP,SAB GTSin 3mn.Top hole SI due to closing of valve
          on flow-head to repair flr li
  DST # 6.  707.7 ~ 713.8m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: Rec. 100' mud. GIP,FAB GTS in 50mn TSTM
  DST # 7.  719.3 ~ 735.8m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: Rec. 95' mud. GIP,GSAB < TO GTS in 1mn
  DST # 8.  734.6 ~ 740.7m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: Rec. 80' mud. WIP, WAB dd in 5mn. ISI false - due to partial tool
          plugging.
  DST # 9.  741.3 ~ 773.3m   Fm: Kfish_brh
     Source:  Government
                               Drill stem test
     RMK: Rec. 195' mud. FIP, FAB > TOT
  DST #10. 1226.8 ~ 1240.5m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 195' mud. GIP, FAB GTS in 45mn VWGB
  DST #11. 1240.5 ~ 1267.4m  Fm: Mhart_rv
     Source:  Government
                               Drill stem test
     RMK: Rec. 100' mud. FIP,VWAB > nil aft tool opend 20mn.
  DST #12. 1289.0 ~ 1304.2m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 190' mud. GIP, GAB > nil in 4mn. Dd aft 15mn. Trouble experienced
          getting thr 16' of tight fil
  DST #13. 1289.3 ~ 1314.9m  Fm: Mchance
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final     217  Mcf/d
     RMK: Rec. 120' clr colorless distillate, 80' gc mud. GIP, GTS before got
          ISI, SGB aft 15mn sl dist cut
  DST #14. 1314.3 ~ 1327.1m  Fm: Mchance
     Source:  Government
                               Drill stem test
     GTS:         Flo:Max           Final     355  Mcf/d
     RMK: Rec. 20' distillate, 10' gc mud. SIP, GTS while shutting ISI SGB @
          15mn.
  DST #15. 1327.1 ~ 1334.1m  Fm: Mchance
     Source:  Government
                               Drill stem test MISRUN
     RMK: Misrun - could not get to btm
  DST #16. 1326.8 ~ 1337.2m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 2000' lg gr oil. GIP, SAB GTS 3mn slwly > TOT
  DST #17. 1337.2 ~ 1345.7m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 10' mud. Tight hole.
  DST #18. 1345.4 ~ 1401.2m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec 2750' but not ment what? GIP, FAB GTS in 15mn TSTM. Had to skid
          13' to btm.
  DST #19. 1487.4 ~ 1540.5m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 4200' swtr. GIP,FAB GTS in 60mn TSTM
  DST #20. 1540.5 ~ 1581.9m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: rec. 950' lt. Oil. GIP, GTS in 2mn
  DST #21. 1565.1 ~ 1586.5m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 490' sl $ gy mud. GIP, GTS in 3mn
  DST #22. 1400.6 ~ 1487.4m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 1500' gy $ swtr. GIP, GTS in 5mn, MTS in 45mn, WTS in 60mn.
  DST #23. 1325.9 ~ 1335.0m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 3bbls mc oil, 4bbls cln oil. GIP, GTS in 17mn
  DST #24. 1581.9 ~ 1586.5m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 18' mud. GIP dd aft ISI resent aft 30mn, dd in 3mn.
  DST #25. 1563.6 ~ 1581.9m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 15' gy mud. GIP, GTS in3mn
  DST #26. 1540.5 ~ 1563.6m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 840' cln lt oil,420' oc mud, 1240' wtr,10M parts per million
          salt. GIP, GTS in 2mn
  DST #27. 1548.4 ~ 1563.6m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 150' cln oil,300' gy oc mud,2175' swtr. GIP, GTS in 3mn TSTM
  DST #28. 1540.5 ~ 1548.4m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 18' mud. GIP, dd aft 70mn
  DST #29. 1555.7 ~ 1563.6m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 30' mud. FIP,dd aft 7mn reset aft 30mn, dd aft 45mn.
  DST #30. 1550.2 ~ 1553.0m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 150' oc mud,150' oil,2120'wtr. GIP,GTS in 14mn
  DST #31. 1586.5 ~ 1621.5m  Fm: Mchance
     Source:  Government
                               Drill stem test MISRUN
     RMK: 210' mud,800' hvy oc mud. GIP,GTS in 1mn TSTM, WGB TOT. Misrun - tool
          not completely opened aft ISI.
  DST #32. 1586.5 ~ 1621.5m  Fm: Mchance
     Source:  Government
                               Drill stem test MISRUN
     RMK: GIP,TAB. Misrun - tool not completely opened aft ISI
  DST #33. 1586.5 ~ 1621.5m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 1400' hvy oc mud,280' oc swtr,1520' swtr. GIP,GTS in 7mn,FGB,
          TSTM TOT
  DST #34. 1667.0 ~ 1685.8m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec.150' mud. GIP,dd aft ISI reset aft 30mn.
  DST #35. 1667.0 ~ 1687.4m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec.450' mud. GIP,GTS in 4mn, TSTM > WGB aft 30mn.
  DST #36. 1726.4 ~ 1738.6m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 15'mud. GIP,dd aft 5mn.
  DST #37. 1754.1 ~ 1776.4m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 1020' mud,4540' s wtr. GIP,GAB > WAB in 15mn, GTS in 20mn VWGB.
  DST #38. 1849.5 ~ 1860.2m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 20' gy mud. GIP,GTS in 4mn TSTM.
  DST #39. 1927.9 ~ 1953.8m  Fm: Mchance
     Source:  Government
                               Drill stem test
     RMK: Rec. 20' gy mud. GIP,GAB > TOT
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  No IP Tests or Production reported.
  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
  Note: Locational information is presented using the NAD27 datum.
